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180GSpecifications
(Material Name180KG Single Door Magnetic Lock


1. Brand and Manufacturer Information
· Manufacturer: Zhongshan Ju'an Shield Electronic Lock Industry Co., Ltd.
· Logo:

2. Material model and version
· Model: 180G
· Version:

3. Main functions and features
          This product is noiseless, wear-free, has no mechanical failures, strong suction, and a longer service life. The lock body is made of selected...
　　　Treated with specialized magnetizing materials and processes, it does not produce residual magnetism during prolonged operation and is not susceptible to magnetism after long-term use.
　　　The magnetization of the plate weakens the suction force. The aluminum material is anodized, while the lock body and suction plate are electroplated to improve adhesion.
　　　It is stronger and has better corrosion resistance.

4. Technical parameters
　    Model: 180G
　    Lock body dimensions: 168×40×21.5(mm)
　    Suction plate dimensions: 140×33×11.5(mm)
　    Working principle: Locks when powered on, unlocks when powered off.
　    Operating voltage: DC 12V ±10%
　    Operating current: 330mA
      Power: 4W
　Operating temperature rise: ≤ Ambient temperature + 15℃
　Static tensile force: 180 kg
  Indicator lights: None
　Operating life: 1 million cycles
　Ambient temperature: -20～55℃
　Lock body materials: silicon steel sheet, pure copper enameled wire, aluminum alloy
　Suction plate material: Electrical pure iron


5. Product view (exterior view)
[image: ]
Model: 180G

6. Product Certification Qualification (Laws and Regulations) Explanation
According to the National Security and Alarm System Product Quality Supervision and Inspection Center (Shanghai)
Testing by the Product Quality Supervision and Inspection Center of the Ministry of Public Security's Security and Alarm System

7. Structural dimension drawing[image: ]

Note: All dimensions are in mm.

8. Bill of Materials
	name
	Quantity (units)

	180G lock body
	1

	Vice board
	1 piece

	M8*30mm mushroom head screw
	1 piece

	M8*50mm Phillips head screw
	1 piece

	M4*30mm Phillips head countersunk screws (for wooden doors)
	5

	Φ20*10*1mm rubber sheet spacer/white gasket
	1

	4.6 cents spoon
	1

	4*12mm spring pin
	2

	manual
	1 copy

	Certificate of Conformity
	1 copy

	Desiccant
	1

	Hole positioning paper
	1 copy



9. Packaging method and outer box labeling
Model: 180G                                                     
    Net weight of a single lock: 1kg                                                       
Total quantity: 24 pieces                                              
Total net weight: 25kg                                                           
Outer box dimensions: 39*21.5*25           
 


Note: Production batch number and production date are subject to the actual goods.

10. Storage and transportation requirements
　　conventional

11. Product warranty and service (optional)
　　Two-year warranty.

All information above is the property of Zhongshan Ju'an Shield Electronic Lock Industry Co., Ltd. and may not be disclosed. 	No.5Page
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